**Knox Western Model TP245 S/N 1352 1200 RPM with 2 single stage 3-1/2” 1500 PSI cylinders and Teco Westinghouse 150 HP electric motor S/N KH C7B104-5**

This package has the following features:

Ronaco 16 ft X 14 ft OD dimension building with 12.6 ft peak to ground height

15.4 ft X 13.4 ft ID wall dimension with 8.6 ft wall height and 11 ft peak

1---36” wide X 35” high aluminum sliding window on one of the 14 ft walls

2---Double Doors close to center of the 16 ft walls 70” wide X 82” high

1---12” exhaust fan Model 4C3458 with ¼ HP 115V 1725 RPM Marathon electric motor mounted above window

1---3 module Premier Model 706903 lubricator with Baldor 1/3 HP 1140 RPM Model M7003A Spec 35E354Z08 electric motor

1---Ruffneck Model HP5-16 natural gas heater

1---Viking pump Model G 90 M with Baldor 1 HP 1725 RPM Model CM7014 Spec 35E368-87 electric motor

1---12” wide X 14” high Oil Cooler

1---Murphy Model VS-2 vibration switch

1---Gas scrubber 12” diameter X 77” high with sight glass MAWP 1290 @ 350 deg F, CRN L1497.2 with Fisher liquid level controller Model 2680A/2681 and Fisher Model 128PQC 1” Dump Valve and Regulator

1---REN 4 US Gal day tank with sight glass

1---Murphy Model LM 303 Crank case oil level controller

1---1” G479 valve Model 14578732 with Fisher 657 Actuator and 0-35 PSI Fisher Regulator

1---Panel with 0-600 PSI / 0-4000 KPA Suction Press Gauge, 0-1500 PSI/0-10000 KPA Discharge Press Gauge and Amot Hawk I Panel Control Model 8630A13301U-3